**CLOVER SYSTEM – 1**

Effortless and stylish square look design.

Bottom track to be placed over finished surface.

Brackets to be mounted in pieces & cover to be fixed in a continuous length.

This system can also be used as a slotted brackets system.

No pre-planning is required as it is a floor mounting system.

Available Glass bracket sizes : 100mm, 125mm, 150mm, 175mm, 200mm, 225mm, 250mm, 275mm & 300mm.

Suitable for glass thickness from 12mm to 17.5mm Laminated and Sentry.

Available in two finishes, Silver and Champagne.